{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["4-2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"4-2","index":0,"n_rows":22,"n_cols":15,"rows_kept":22,"cut":false,"hidden":false,"merged":[[18,0,18,14],[11,12,12,12],[11,13,12,13],[11,14,12,14],[11,6,12,6],[11,7,12,7],[11,8,12,8],[11,9,12,9],[11,10,12,10],[11,11,12,11],[11,0,12,0],[11,1,12,1],[11,2,12,2],[11,3,12,3],[11,4,12,4],[11,5,12,5],[7,13,8,13],[5,13,6,13],[5,14,6,14],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,14,8,14],[7,9,8,9],[7,10,8,10],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,9,6,9],[5,10,6,10],[20,0,20,14],[21,0,21,13],[19,0,19,14],[13,9,14,9],[13,10,14,10],[13,11,14,11],[13,0,14,0],[13,1,14,1],[13,2,14,2],[1,10,1,14],[2,9,3,10],[2,13,3,14],[2,1,3,2],[2,3,3,4],[2,11,3,12],[0,0,0,8],[2,0,4,0],[5,11,6,11],[5,12,6,12],[7,11,8,11],[7,12,8,12],[5,7,6,7],[5,8,6,8],[2,5,3,6],[2,7,3,8],[13,3,14,3],[13,4,14,4],[13,12,14,12],[13,13,14,13],[13,14,14,14],[13,5,14,5],[13,6,14,6],[13,7,14,7],[13,8,14,8],[5,5,6,5],[5,6,6,6],[7,5,8,5],[7,6,8,6],[7,7,8,7],[7,8,8,8],[9,6,10,6],[9,7,10,7],[9,0,10,0],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,10,4],[9,5,10,5],[9,14,10,14],[9,8,10,8],[9,9,10,9],[9,10,10,10],[9,11,10,11],[9,12,10,12],[9,13,10,13],[15,0,16,0],[15,1,16,1],[15,2,16,2],[15,3,16,3],[15,4,16,4],[15,5,16,5],[15,12,16,12],[15,13,16,13],[15,14,16,14],[15,6,16,6],[15,7,16,7],[15,8,16,8],[15,9,16,9],[15,10,16,10],[15,11,16,11]],"flags":["formulas_cached_only"]}
["４－２　電気事業用発電設備（道内）"]
[{"$nulls":10},"（単位：1,000kW、％）"]
["年度末","水　　　力",null,"火　　　力",null,"原　子　力",null,"風力",null,"太陽光",null,"地熱",null,"合　　　計"]
[]
[null,"最大出力","構成比","最大出力","構成比","最大出力","構成比","最大出力","構成比","最大出力","構成比","最大出力","構成比","最大出力","構成比"]
["平成26",1657,20.121432908318155,4482,54.42622950819672,2070,25.136612021857925,0,0,1,0.012143290831815423,25,0.3035822707953855,8235,100]
[]
["平成27",1863,22.070844686648503,4482,53.09797417367611,2070,24.52316076294278,0,0,1,0.011846937566639024,25,0.2961734391659756,8441,100]
[]
["平成28",1648,20.711323363076538,4214,52.9596581626241,2070,26.01482970968958,0,0,1,0.012567550584391103,25,0.3141887646097775,7957,100.0125675505844]
[]
["平成29",1648,21.101152368758,4065,52.04865556978233,2070,26.504481434058896,0,0,1,0.012804097311139564,25,0.3201024327784891,7810,99.98719590268885]
[]
["平成30",1650,19.687388139840113,4635,55.30366304736904,2070,24.69872330270851,0,0,1,0.011931750387781888,25,0.2982937596945472,8381,99.99999999999999]
[]
["平成31\n（令和元）",1651,19.696969696969695,4635,55.297065139584824,2070,24.695776664280604,0,0,1,0.011930326890956812,25,0.29825817227392026,8382,100]
[]
[{"$nulls":11}," "]
["出所：H26～H27 電気事業便覧（電気事業連合会）　北海道電力（株）と電源開発（株）分の合計値を掲載\n        H28～H31 電力統計情報（電気事業連合会）　北海道電力（株）分のみを掲載"]
["(注)　1.火力には地熱を含む。"]
["     　2.火力と石炭＋石油の差は内燃力、ガスタービン等である。"]
["　　 　3.（　）内は苫小牧共同火力（25万kW　3基）の1/2、37万5,000kWを除いた値である。"]